Firewire IEEE 1394

Brouillon

Canon HDV LEGRIA HV40

Voir FIXME2

Kino

Kdenlive

dvgrab

#!/bin/bash # # 2013-01-23 # # This script allows the video/audio streaming of the Canon Legria HV40 # connected via 1394/firewire on an Alienware Mx11R3 # It can be started on a Ubuntu Precise Live System # # Dependencies: vlc dvgrab # sudo bash -c "echo ' deb http://archive.ubuntu.com/ubuntu/ precise main restricted universe multiverse deb http://security.ubuntu.com/ubuntu/ precise-security main restricted universe multiverse deb http://archive.ubuntu.com/ubuntu/ precise-updates main restricted universe multiverse ' > /etc/apt/sources.list" sudo apt-get update sudo apt-get install -y dvgrab vlc ffmpeg libavcodec-extra-53 htop openssh-server dvgrab -autosplit -frames 0 -size 0 -format hdv -buffers 1000 - | cvlc - --no-sub-autodetect-file --sout '#transcode {vcodec=theo,vb=800,scale=0.25,acodec=mp3,ab=128,channels=2,samplerate=44100} :http{mux=ogg,dst=:8080/}'

Source https://gist.github.com/jfbucas/4608578